

Hi Fi Simulator Preparation Check List

* Check battery charging indicator status on charger
* Disconnect charger (power supply can be kept connected for Newborns)
* Prepare simulated blood / urine / medication (use distilled water)
* Prepare equipment / consumables requested
* UNI Launch / Connection established
* Monitor Launch / Connection established
* Debriefing system launch/ connection established:
* Check breathing / pulses / blinking
* Prime drug recognition system (Distilled water only)
* Fill fluid containers with prepared solutions
* Review Palettes / Scenarios
* Lubrication: Airway (ET tube only), Birthing mechanism, fetus & placenta
* Run a diagnostic test

Hi Fi Simulator Post-Session Check List

* Connect charger and check indicator status
* Drain all remaining fluids (PPH, Urine and IV…): Flush with Distilled Water & 70% Alcohol from time to time
* Remove consumables (IV, moulage, ETT & Patches)
* Clean with cloth and diluted dish-washing soap
* Reset the birthing simulator / dynamic lungs
* Save wanted palettes, scenarios and logs
* Check for software updates
* Shutdown UNI/ Monitors and computers
* Store the fetus outside the birthing mechanism
* Cover & Store in recommended conditions

Prepared by Carlos Chidiac, MD – Gaumard Middle East & N. Africa - **intlsales@gaumard.com**